{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":4,"rows_kept":36,"merged":[[0,0,0,3],[1,0,1,3],[2,0,2,3],[4,0,4,3],[18,0,18,3],[30,0,30,3],[35,0,36,3]],"flags":["formulas_cached_only"]}
["商用车维护作业表（选手记录表）"]
["选手参赛号:                                           裁判签字：                   "]
["车型：                                                       VIN："]
["个性化\n顺序号","项目编号","作业类型+作业对象+作业内容","记录内容"]
["车辆未举升作业项目"]
[null,"001","作业准备\n- 安装车轮挡块 、比赛车辆的检查                                               "]
[null,"002","作业准备                                                 \n- 作业工量具检查"]
[null,"003","作业准备                                                 \n- 在维修工单内记录车辆识别号"]
[null,"004","检查作业\n- 驻车制动效能（施加驻车制动时通过弹簧气室是否有排气声判断）"]
[null,"005","检查作业\n-通过施加、释放驻车制动检查制动报警灯工作状态"]
[null,"006","检查作业                                                  \n- 检查制动液和离合器液位和品质"]
[null,"007","检查作业\n-测量制动踏板自由行程","制动踏板自由行程："]
[null,"008","检查作业\n-测量离合器踏板自由行程","离合器踏板自由行程："]
[null,"009","检查作业\n-检查离合器总泵进出油管及固定情况"]
[null,"010","检查作业\n- 检查变速箱气管路；\n- 检查变速器通气塞状况\n"]
[null,"011","转向盘最大自由转动量\n- 测量转向盘最大自由转动量","转向盘最大自由转动量：\n结果判断：□正常，□异常"]
[null,"012","车辆前部及部分底盘线束\n- 检查车头前部线束、蓄电池电缆和油箱上部线束及其连接器"]
[null,"013","车轮及轮胎\n- 前轴两侧轮胎一致性检查\n- 备胎花纹深度测量\n- 并装双胎安装状态检查","\n\n\n轮胎花纹深度："]
["车辆举升后作业项目"]
[null,"014","储气筒、干燥器及管路\n- 检查储气筒固定情况\n- 检查储气筒内是否有水分\n- 检查制动管路固定及泄漏情况"]
[null,"015","制动调整臂\n- 全车制动调整臂自动调整装置、自锁装置及调整臂连接情况检查"]
[null,"016","转向器\n- 检查转向器固定和连接器状况"]
[null,"017","转向传动机构\n- 检查转向传动机构（横直拉杆及球头）状态"]
[null,"018","车桥\n- 检查前桥自动调整臂有效性；\n- 测量前桥自动调整臂轴向间隙；\n- 检查中桥主减速器齿轮油油量和品质；\n- 检查检查中桥主减速器通气塞有效性；\n- 调整后桥自动调整臂间隙。"]
[null,"019","前悬架\n- 检查前减震器\n- 检查前稳定杆\n- 检查检查钢板弹簧夹与钢板弹簧的间隙，以及缓冲间隙","\n\n\n弹簧夹与钢板弹簧的间隙：\n缓冲间隙："]
[null,"020","后悬架\n- 检查检查钢板弹簧夹与钢板弹簧的间隙，以及缓冲间隙\n- 检查V型推力杆外观和固定情况","弹簧夹与钢板弹簧的间隙：\n缓冲间隙：\n\n"]
[null,"021","离合器\n- 检查离合助力器排气口工作情况\n- 检查离合分泵助力器进油、进气管固定及泄漏情况"]
[null,"022","变速器\n- 检查变速箱齿轮油液面和品质；\n- 检查变速箱与发动机和传动轴的连接情况；\n"]
[null,"023","传动轴\n- 目视检查传动轴总成；\n- 检查中间传动轴固定情况；\n- 检查中间传动轴轴承。"]
[null,"024","底盘线束及导线\n- 检查底盘线束和导线连接情况"]
["车辆落地后作业项目"]
[null,"025","蓄电池\n- 测量蓄电池外观检查；\n- 测量蓄电池电压。","外观：\n蓄电池电压："]
[null,"026","尿素溶液\n- 检查尿素罐液位；\n- 测量尿素检测仪测量尿素的浓度","液位：\n浓度："]
[null,"027","灯光\n- 检查前照灯、转向灯、示廓灯、制动灯和倒车灯工作情况"]
[null,"028","整理作业\n- 取下车轮挡块归位、清洁车辆                                                             \n"]
["发现异常情况以及相关测量数据，在“记录内容”栏内记录；若正常请在记录内容栏目内打“√”。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}