{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["检查程序"],"not_rendered":{"images":6,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"检查程序","index":0,"n_rows":16,"n_cols":13,"rows_kept":16,"merged":[[3,1,3,12],[5,2,5,3],[5,4,5,5],[5,6,5,7],[5,8,5,9],[5,10,5,11],[6,2,6,3],[6,4,6,5],[6,6,6,7],[6,8,6,9],[6,10,6,11],[8,1,15,1],[8,3,15,3],[8,5,15,5],[8,7,15,7],[8,9,15,9],[8,11,15,11]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"2016年定期维护作业流程——举升位置图"]
[]
[null,"编号",1,null,2,null,3,null,4,null,5,null,6]
[null,"顶起位置"]
[]
[null,"主要\n作业\n内容","标记燃油量和车辆损毁部位及类型",null,"排放发动机机油",null,"检查左前减振器",null,"紧固左侧车轮螺母",null,"检查机油泄漏",null,"尾气分析仪归位"]
[null,null,"检查发动机冷却、润滑、制动、玻璃清洗液液位",null,"检查发动机冷却、润滑、燃油系统和制动系统泄漏、损坏、安装",null,"测量左后轮胎花纹深度",null,"更换机油滤清器、空气滤清器",null,"检查冷却液泄漏",null,"检查发动机机油液位"]
[null,null,"检查冷却液冰点；进行水箱盖和冷却系统压力测试",null,"检查驱动轴护套",null,"拆装左侧车轮并前后换位",null,"加注发动机机油",null,"检查制动液泄漏",null,"检查制动液液位"]
[null,null,"检查蓄电池、喇叭、灯光、仪表、刮水器、洗涤器",null,"检查转向横拉杆防尘罩",null,"拆装检查左前制动器，更换左前制动片",null,"检查制动助力器助力能力",{"$nulls":3},"工具设备归位"]
[null,null,"检测发动机故障码",null,"检查排气系统泄漏、损伤、脱落或缺失情况",null,"拆装检查左后制动器",null,"检查右后视镜",{"$nulls":3},"车身防护用品归位"]
[null,null,"检查制动感觉、转向柱调整、安全带回收、备胎气压",null,"紧固前副车架螺栓",null,"测量制动踏板自由行程和行程",null,"进行充电系统测试",{"$nulls":3},"车身内外清洁"]
[null,null,"检查发动机舱盖锁、行李箱盖锁、左后车门锁",null,"紧固后减振器螺栓",null,"测量驻车制动拉杆行程",null,"检查空调风向切换和制冷"]
[null,null,"检查换挡杆及挡位指示灯",null,"安装油底壳放油螺塞",null,"启动尾气分析仪",null,"检测尾气"]