{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["选手1作业表","选手2作业表"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"选手1作业表","index":0,"n_rows":147,"n_cols":7,"rows_kept":147,"merged":[[0,0,0,5],[2,0,2,1],[4,0,4,5],[59,0,59,5],[80,0,80,5],[115,0,115,5],[133,0,133,5],[137,0,137,5],[146,0,148,1],[146,2,148,5],[146,6,148,6]],"flags":["formulas_cached_only"]}
["           2016年全国中等职业学校“上汽通用”杯汽车运用与维修技能大赛团体定期维护项目作业表"]
[]
["选手号:                ",{"$nulls":3},"选手姓名:                                 裁判员签字:  "]
["选手1顺序","合作项目顺序","记录项","项目编号","作业类型+作业对象+作业内容","说明","扣分"]
["以下是顶起位置1"]
[{"$nulls":3},"001","作业准备- 安全防护                                            \n- 拉紧驻车制动杆，并将换挡杆置于P位置"]
[{"$nulls":3},"002","作业准备- 安全防护                                                \n- 安装车轮挡块"]
[null,null,"填写附表","003","作业准备- 车身                                                  \n- 在维修工单内记录车辆识别号"]
[null,null,"填写附表","004","检查作业- 车身                                                  \n- 检查并标记车辆损毁位置及损毁类型"]
[{"$nulls":3},"005","作业准备- 安全防护                                                  \n- 安装座椅套、方向盘套和地板垫"]
[{"$nulls":3},"006","作业准备- 安全防护                                               \n- 安装翼子板布和前格栅布"]
[null,null,"填写附表","007","检查作业- 发动机冷却系统                                               \n- 检查发动机冷却液液位"]
[null,null,"填写附表","008","检查作业- 发动机冷却系统\n- 测量并记录发动机冷却液冰点"]
[null,null,"填写附表","009","检查作业- 发动机冷却系统\n- 进行水箱盖压力测试"]
[null,null,"填写附表","010","检查作业- 发动机冷却系统\n- 进行冷却系统压力测试并检查冷却水管及接口有无泄漏"]
[{"$nulls":3},"011","检查作业- 发动机冷却系统\n- 检查冷却水管的安装情况及有无裂纹、凸起、硬化、磨损或其他损坏"]
[null,null,"填写附表","012"," 检查作业- 制动系统                                               \n- 检查制动液液位，必要时调整"]
[null,null,"填写附表","013","检查作业- 挡风玻璃洗涤器                                              \n- 检查前挡风玻璃洗涤液液位"]
[null,null,"填写附表","014","检查作业- 发动机润滑系统                                                \n- 检查发动机机油液位"]
[{"$nulls":3},"015","检查作业- 电源系统\n- 检查蓄电池的安装、污染及损坏情况"]
[{"$nulls":3},"016","检查作业- 电源系统\n- 检查蓄电池连接端子有无腐蚀、松动"]
[null,null,"填写附表","017","检查作业- 电源系统\n- 测量并记录蓄电池电压（静态）","发动机熄火"]
[{"$nulls":3},"018","检查作业- 制动系统                 \n- 检查制动踏板踩下时的行程和感觉"]
[{"$nulls":3},"019","检查作业- 喇叭                                       \n- 检查喇叭按钮及喇叭的工作情况"]
[null,null,"填写附表","020","作业准备- 组合仪表                                                  \n- 在维修工单内标记燃油量"]
[{"$nulls":3},"021","检查作业- 组合仪表\n- 检查MIL、AIRBAG、ABS故障指示灯和充电、机油压力报警灯的工作情况 "]
[{"$nulls":3},"022","检查作业- 组合仪表\n- 检查驻车制动器指示灯的工作情况"]
[{"$nulls":3},"023","检查作业- 组合仪表\n- 检查组合仪表背景灯的亮度调节功能"]
[null,null,"填写附表","024","检测作业- 发动机控制\n- 检测并记录发动机系统故障码"]
[{"$nulls":3},"025","检查作业- 车外灯\n- 检查前部示宽灯的工作情况"]
[{"$nulls":3},"026","检查作业- 车外灯/组合仪表                                         \n- 检查前部转向灯（含侧面）及其指示灯的工作情况 "]
[{"$nulls":3},"027","检查作业- 转向灯开关                                             \n- 检查转向信号/多功能开关的自动返回功能"]
[{"$nulls":3},"028","检查作业- 车外灯/组合仪表                                           \n- 检查前部危险警告灯（含侧面）及其指示灯的工作情况"]
[{"$nulls":3},"029","检查作业- 车外灯\n- 检查前照灯近光的工作情况","起动发动机"]
[{"$nulls":3},"030","检查作业- 车外灯/组合仪表\n- 检查前照灯远光及其指示灯的工作情况","起动发动机"]
[{"$nulls":3},"031","检查作业- 车外灯/组合仪表\n- 检查前照灯闪光及远光指示灯的工作情况","起动发动机"]
[{"$nulls":3},"032","检查作业- 车外灯\n- 检查后部示宽灯的工作情况"]
[{"$nulls":3},"033","检查作业- 车外灯 \n- 检查后部转向灯的工作情况 "]
[{"$nulls":3},"034","检查作业- 车外灯/组合仪表                                           \n- 检查后部危险警告灯及其指示灯的工作情况"]
[{"$nulls":3},"035","检查作业- 车外灯\n- 检查牌照灯的工作情况"]
[{"$nulls":3},"036","检查作业- 车外灯\n- 检查制动灯（含高位）的工作情况"]
[{"$nulls":3},"037","检查作业- 车外灯\n- 检查倒车灯的工作情况","发动机熄火"]
[{"$nulls":3},"038","检查作业- 前挡风玻璃洗涤器\n- 检查前挡风玻璃洗涤器的喷射力和喷射位置","目测"]
[{"$nulls":3},"039","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃洗涤器喷射时刮水器的联动情况"]
[{"$nulls":3},"040","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的低速工作情况及有无异响"]
[{"$nulls":3},"041","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的高速工作情况及有无异响"]
[{"$nulls":3},"042","检查作业- 前挡风玻璃刮水器 \n-  检查前挡风玻璃刮水器的自动回位功能"]
[{"$nulls":3},"043","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的刮拭情况"]
[{"$nulls":3},"044","检查作业- 转向系统\n- 检查转向柱的倾斜调整及锁止情况"]
[{"$nulls":3},"045","检查作业- 安全带　　　　                                    \n- 检查驾驶员座椅安全带的拉伸和卷收情况及安全带有无撕裂或磨损"]
[{"$nulls":3},"046","检查作业- 安全带　　　　                                     \n- 检查驾驶员座椅安全带惯性开关和安全带扣锁止开关的工作情况"]
[{"$nulls":3},"047","拆装作业- 发动机                                                    \n- 拆下机油加注口盖"]
[{"$nulls":3},"048","检查作业- 发动机舱盖                                                       \n- 检查发动机舱盖锁和微开开关的工作情况"]
[{"$nulls":3},"049","检查作业- 车门      \n- 检查左后车门门锁（含儿童锁）和微开开关的工作情况"]
[{"$nulls":3},"050","检查作业- 车内灯                                                      \n- 检查行李箱照明灯是否点亮"]
[{"$nulls":3},"051","检查作业- 行李箱盖                               \n- 检查行李箱盖锁和微开开关的工作情况"]
[null,null,"填写附表","052","检查作业- 轮胎                                                   \n- 检测备用轮胎气压及轮胎是否漏气，必要时调整气压"]
[{"$nulls":3},"053","检查作业- 自动变速器\n- 检查换挡杆及挡位指示灯的工作情况，检查完毕后将换档杆置于N位置"]
[{"$nulls":3},"054","作业准备- 制动系统\n- 释放驻车制动杆"]
["以下是顶起位置2"]
[{"$nulls":3},"055","检查作业- 发动机 \n- 检查发动机各油封及结合面有无漏油 "]
[{"$nulls":3},"056","检查作业- 发动机\n- 检查机油滤清器及油底壳放油螺塞有无漏油"]
[{"$nulls":3},"057","拆装作业- 发动机润滑系统\n- 排放发动机机油"]
[{"$nulls":3},"058","检查作业- 发动机冷却系统                            \n- 检查散热器有无泄漏、脏污、变形或损坏"]
[{"$nulls":3},"059","检查作业- 传动系统\n- 检查左驱动轴护套有无泄漏、裂纹或损坏（外侧）"]
[{"$nulls":3},"060","检查作业- 传动系统\n- 检查右驱动轴护套有无泄漏、裂纹或损坏（外侧）"]
[{"$nulls":3},"061","检查作业- 转向系统\n- 检查左转向横拉杆防尘罩有无漏油、裂纹或损坏"]
[{"$nulls":3},"062","检查作业- 转向系统\n- 检查右转向横拉杆防尘罩有无漏油、裂纹或损坏"]
[{"$nulls":3},"063","检查作业- 燃油供给系统\n- 检查燃油管及接头有无泄漏"]
[{"$nulls":3},"064","检查作业- 燃油供给系统\n- 检查燃油管的安装情况及有无扭结、磨损、腐蚀或其他损坏"]
[{"$nulls":3},"065","检查作业- 制动系统\n- 检查制动管及接头有无泄漏"]
[{"$nulls":3},"066","检查作业- 制动系统\n- 检查制动管的安装情况及有无扭结、磨损、腐蚀或其他损坏"]
[{"$nulls":3},"067","检查作业- 排气系统\n- 检查三元催化器、排气管、消声器有无凹陷、刮伤、腐蚀或其他损坏"]
[{"$nulls":3},"068","检查作业- 排气系统\n- 检查排气系统各密封垫片有无泄漏"]
[{"$nulls":3},"069","检查作业- 排气系统\n- 检查排气管、消声器的吊挂有无裂纹、损坏、脱落或缺失"]
[{"$nulls":3},"070","紧固作业- 前副车架\n- 紧固前副车架与车身连接螺栓（后部）"]
[{"$nulls":3},"071","紧固作业- 后桥托架\n- 紧固后桥托架与车身连接螺栓（内侧）"]
[{"$nulls":3},"072","固作业- 后悬架\n- 紧固左后减振器下螺栓"]
[{"$nulls":3},"073","紧固作业- 后悬架\n- 紧固右后减振器下螺栓"]
[{"$nulls":3},"074","拆装作业- 发动机\n- 更换新的放油螺塞密封件并安装放油螺塞"]
["以下是顶起位置3"]
[{"$nulls":3},"075","检查作业- 前悬架                                                  \n- 检查左前减振器有无漏油、变形或其他损坏"]
[{"$nulls":3},"076","检查作业- 车轮\n- 检查左前车轮轴承有无松旷和异响"]
[{"$nulls":3},"077","拆装作业- 车轮\n- 拆卸左前车轮"]
[{"$nulls":3},"078","拆装作业- 制动系统 \n- 拆卸左前轮制动钳下部固定螺栓"]
[{"$nulls":3},"079","检查作业- 制动系统 \n- 检查左前轮制动钳导销是否松旷、导销护套有无裂纹或损坏"]
[{"$nulls":3},"080","检查作业- 制动系统\n- 检查左前轮制动钳活塞有无泄漏"]
[{"$nulls":3},"081","拆装作业- 制动系统\n- 用专用工具压回左前轮制动钳活塞"]
[{"$nulls":3},"082","拆装作业- 制动系统 \n- 拆卸并检查左前轮制动片固定弹簧有无变形、裂纹或损坏"]
[{"$nulls":3},"083","检查作业- 制动系统\n- 检查左前轮制动盘有无裂纹、沟槽或损坏"]
[null,null,"填写附表","084","检测作业- 制动系统 \n- 测量并记录左前轮制动盘横向跳动量"]
[{"$nulls":3},"085","拆装作业- 制动系统\n- 安装左前轮制动片固定弹簧"]
[{"$nulls":3},"086","拆装作业- 制动系统\n- 更换左前轮制动片"]
[{"$nulls":3},"087","拆装作业- 制动系统\n- 安装左前轮制动钳"]
[null,null,"填写附表","088","检测作业- 轮胎                                                    \n-检测并记录左后轮胎胎面沟槽深度"]
[{"$nulls":3},"089","拆装作业- 车轮\n- 拆下左后车轮总成"]
[{"$nulls":3},"090","拆装作业- 制动系统\n- 拆下左后轮制动鼓螺钉并取下制动鼓"]
[{"$nulls":3},"091","检查作业- 制动系统\n- 检查左后轮制动鼓表面状况"]
[null,null,"填写附表","092","检测作业- 制动系统\n- 测量并记录左后轮制动鼓直径"]
[{"$nulls":3},"093","检查作业- 制动系统 \n- 检查左后轮制动分泵有无漏油、护套有无裂纹和损坏"]
[{"$nulls":3},"094","检查作业- 制动系统 \n- 检查左后轮制动分泵活塞有无卡滞"]
[{"$nulls":3},"095","检查作业- 制动系统\n- 检查左后轮制动蹄摩擦衬片有无裂纹、缺损和油污"]
[null,null,"填写附表","096","检测作业- 制动系统\n- 测量并记录左后轮制动蹄直径，并计算其与制动鼓的间隙"]
[{"$nulls":3},"097","检查作业- 制动系统\n- 检查左后轮制动器调节弹簧有无缺失、弯曲、裂纹或严重锈蚀"]
[{"$nulls":3},"098","检查作业- 制动系统 \n- 检查左后轮制动器调节器总成有无弯曲、裂纹、过度磨损、损坏或缺齿"]
[{"$nulls":3},"099","拆装作业- 制动系统 \n- 安装左后轮制动鼓并紧固制动鼓螺钉"]
[{"$nulls":3},"100","调整作业- 制动系统\n- 恢复制动器盘片和蹄鼓的间隙"]
[{"$nulls":3},"101","检查作业- 制动系统                                                              \n- 检查左前制动盘转动是否灵活"]
[{"$nulls":3},"102","拆装作业- 制动系统                                                    \n- 进行左侧车轮前后换位，安装并预紧固左前车轮"]
[{"$nulls":3},"103","检查作业- 制动系统                                                              \n- 检查左后制动鼓转动是否灵活"]
[{"$nulls":3},"104","拆装作业- 制动系统                                                    \n- 进行左侧车轮前后换位，安装并预紧固左后车轮"]
[null,null,"填写附表","105","检查作业- 制动系统                                              \n- 检查并记录制动踏板的自由行程"]
[null,null,"填写附表","106","检查作业- 制动系统                                            \n- 检查并记录制动踏板的行程"]
[null,null,"填写附表","107","检查作业- 制动系统\n- 检查并记录驻车制动器拉杆的行程"]
[{"$nulls":3},"108","作业准备- 工量具和设备\n- 启动尾气分析仪                 "]
["以下是顶起位置4"]
[{"$nulls":3},"109","作业准备- 安全防护                                            \n- 拉紧驻车制动杆，并将换挡杆置于P位置"]
[{"$nulls":3},"110","作业准备- 安全防护\n- 安装车轮挡块"]
[{"$nulls":3},"111","紧固作业- 车轮             \n- 紧固左前车轮螺母","扭矩为80NM"]
[{"$nulls":3},"112","紧固作业- 车轮             \n- 紧固左后车轮螺母","扭矩为80NM"]
[{"$nulls":3},"113","拆装作业- 发动机润滑系统\n- 拆卸机油滤清器盖及其密封件"]
[{"$nulls":3},"114","拆装作业- 发动机润滑系统\n- 更换新的机油滤清器芯"]
[{"$nulls":3},"115","拆装作业- 发动机润滑系统 \n- 更换新的机油滤清器盖密封件并安装机油滤清器盖"]
[null,null,"填写附表","116","拆装作业- 发动机润滑系统\n- 加注新的发动机油并填写发动机机油更换记录表"]
[{"$nulls":3},"117","检查作业- 进气系统\n- 检查并清洁空气滤清器外壳"]
[{"$nulls":3},"118","拆装作业- 进气系统\n- 更换新的空气滤清器芯"]
[{"$nulls":3},"119","作业准备- 发动机\n- 起动发动机并暖机(及时观察发动机机油有无泄漏)"]
[{"$nulls":3},"120","检查作业- 制动系统                                          \n- 检查制动助力器的助力能力"]
[{"$nulls":3},"121","检查作业- 玻璃升降器                        \n- 检查主控制开关的玻璃升降控制功能","起动发动机"]
[{"$nulls":3},"122","检查作业- 车外后视镜                         \n- 检查右后视镜的调整功能"]
[{"$nulls":3},"123","检查作业- 空调\n- 检查风速调节和风向切换功能以及制冷系统能否工作","起动发动机"]
[null,null,"填写附表","124","检查作业- 电源系统\n- 进行充电系统测试，并记录蓄电池充电电压"]
[null,null,"填写附表","125","检测作业- 发动机排气系统 \n- 检测并记录发动机怠速时的尾气排放值"]
["以下是顶起位置5"]
[{"$nulls":3},"126","检查作业- 发动机                                                              \n- 检查发动机机油有无泄漏"]
[{"$nulls":3},"127","检查作业- 发动机                                                              \n- 检查冷却液有无泄漏"]
[{"$nulls":3},"128","检查作业- 制动系统                                                               \n- 检查左前和左后部有无制动液泄漏"]
["以下是顶起位置6"]
[{"$nulls":3},"129","整理作业- 工量具和设备\n- 关闭尾气分析仪并清洁归位"]
[{"$nulls":3},"130","检查作业- 发动机润滑系统\n- 检查发动机机油液位，必要时调整"]
[{"$nulls":3},"131","整理作业- 工量具和设备\n- 清洁工量具和设备并归位"]
[{"$nulls":3},"132","整理作业- 安全防护                                                               \n- 拆卸翼子板布和前格栅布"]
[{"$nulls":3},"133","整理作业- 安全防护                                                               \n- 拆卸座椅套、地板垫、方向盘套"]
[{"$nulls":3},"134","清洁作业- 车身                                                              \n- 清洁车辆内部、烟灰缸等"]
[{"$nulls":3},"135","清洁作业- 车身                                                              \n- 清洁车辆外表"]
[]
["说明：",null,"对于不合格的作业项目，要在维修工单内写明故障点，并勾选相应的维修措施；记录项划斜杠的，无需记录；记录项中标明填写附表的，按附表的要求填写。"]

{"sheet":"选手2作业表","index":1,"n_rows":147,"n_cols":7,"rows_kept":147,"merged":[[0,0,0,5],[2,0,2,1],[4,0,4,5],[59,0,59,5],[80,0,80,5],[115,0,115,5],[133,0,133,5],[137,0,137,5],[146,0,148,1],[146,2,148,5],[146,6,148,6]],"flags":["formulas_cached_only"]}
["           2016年全国中等职业学校“上汽通用”杯汽车运用与维修技能大赛团体定期维护项目作业表"]
[]
["选手号:                ",{"$nulls":3},"选手姓名:                                 裁判员签字:  "]
["选手2顺序","合作项目顺序","记录项","项目编号","作业类型+作业对象+作业内容","说明","扣分"]
["以下是顶起位置1"]
[{"$nulls":3},"001","作业准备- 安全防护                                            \n- 拉紧驻车制动杆，并将换挡杆置于P位置"]
[{"$nulls":3},"002","作业准备- 安全防护                                                \n- 安装车轮挡块"]
[null,null,"填写附表","003","作业准备- 车身                                                  \n- 在维修工单内记录车辆识别号"]
[null,null,"填写附表","004","检查作业- 车身                                                  \n- 检查并标记车辆损毁位置及损毁类型"]
[{"$nulls":3},"005","作业准备- 安全防护                                                  \n- 安装座椅套、方向盘套和地板垫"]
[{"$nulls":3},"006","作业准备- 安全防护                                               \n- 安装翼子板布和前格栅布"]
[null,null,"填写附表","007","检查作业- 发动机冷却系统                                               \n- 检查发动机冷却液液位"]
[null,null,"填写附表","008","检查作业- 发动机冷却系统\n- 测量并记录发动机冷却液冰点"]
[null,null,"填写附表","009","检查作业- 发动机冷却系统\n- 进行水箱盖压力测试"]
[null,null,"填写附表","010","检查作业- 发动机冷却系统\n- 进行冷却系统压力测试并检查冷却水管及接口有无泄漏"]
[{"$nulls":3},"011","检查作业- 发动机冷却系统\n- 检查冷却水管的安装情况及有无裂纹、凸起、硬化、磨损或其他损坏"]
[null,null,"填写附表","012"," 检查作业- 制动系统                                               \n- 检查制动液液位，必要时调整"]
[null,null,"填写附表","013","检查作业- 挡风玻璃洗涤器                                              \n- 检查前挡风玻璃洗涤液液位"]
[null,null,"填写附表","014","检查作业- 发动机润滑系统                                                \n- 检查发动机机油液位"]
[{"$nulls":3},"015","检查作业- 电源系统\n- 检查蓄电池的安装、污染及损坏情况"]
[{"$nulls":3},"016","检查作业- 电源系统\n- 检查蓄电池连接端子有无腐蚀、松动"]
[null,null,"填写附表","017","检查作业- 电源系统\n- 测量并记录蓄电池电压（静态）","发动机熄火"]
[{"$nulls":3},"018","检查作业- 制动系统                 \n- 检查制动踏板踩下时的行程和感觉"]
[{"$nulls":3},"019","检查作业- 喇叭                                       \n- 检查喇叭按钮及喇叭的工作情况"]
[null,null,"填写附表","020","作业准备- 组合仪表                                                  \n- 在维修工单内标记燃油量"]
[{"$nulls":3},"021","检查作业- 组合仪表\n- 检查MIL、AIRBAG、ABS故障指示灯和充电、机油压力报警灯的工作情况 "]
[{"$nulls":3},"022","检查作业- 组合仪表\n- 检查驻车制动器指示灯的工作情况"]
[{"$nulls":3},"023","检查作业- 组合仪表\n- 检查组合仪表背景灯的亮度调节功能"]
[null,null,"填写附表","024","检测作业- 发动机控制\n- 检测并记录发动机系统故障码"]
[{"$nulls":3},"025","检查作业- 车外灯\n- 检查前部示宽灯的工作情况"]
[{"$nulls":3},"026","检查作业- 车外灯/组合仪表                                         \n- 检查前部转向灯（含侧面）及其指示灯的工作情况 "]
[{"$nulls":3},"027","检查作业- 转向灯开关                                             \n- 检查转向信号/多功能开关的自动返回功能"]
[{"$nulls":3},"028","检查作业- 车外灯/组合仪表                                           \n- 检查前部危险警告灯（含侧面）及其指示灯的工作情况"]
[{"$nulls":3},"029","检查作业- 车外灯\n- 检查前照灯近光的工作情况","起动发动机"]
[{"$nulls":3},"030","检查作业- 车外灯/组合仪表\n- 检查前照灯远光及其指示灯的工作情况","起动发动机"]
[{"$nulls":3},"031","检查作业- 车外灯/组合仪表\n- 检查前照灯闪光及远光指示灯的工作情况","起动发动机"]
[{"$nulls":3},"032","检查作业- 车外灯\n- 检查后部示宽灯的工作情况"]
[{"$nulls":3},"033","检查作业- 车外灯 \n- 检查后部转向灯的工作情况 "]
[{"$nulls":3},"034","检查作业- 车外灯/组合仪表                                           \n- 检查后部危险警告灯及其指示灯的工作情况"]
[{"$nulls":3},"035","检查作业- 车外灯\n- 检查牌照灯的工作情况"]
[{"$nulls":3},"036","检查作业- 车外灯\n- 检查制动灯（含高位）的工作情况"]
[{"$nulls":3},"037","检查作业- 车外灯\n- 检查倒车灯的工作情况","发动机熄火"]
[{"$nulls":3},"038","检查作业- 前挡风玻璃洗涤器\n- 检查前挡风玻璃洗涤器的喷射力和喷射位置","目测"]
[{"$nulls":3},"039","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃洗涤器喷射时刮水器的联动情况"]
[{"$nulls":3},"040","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的低速工作情况及有无异响"]
[{"$nulls":3},"041","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的高速工作情况及有无异响"]
[{"$nulls":3},"042","检查作业- 前挡风玻璃刮水器 \n-  检查前挡风玻璃刮水器的自动回位功能"]
[{"$nulls":3},"043","检查作业- 前挡风玻璃刮水器\n- 检查前挡风玻璃刮水器的刮拭情况"]
[{"$nulls":3},"044","检查作业- 转向系统\n- 检查转向柱的倾斜调整及锁止情况"]
[{"$nulls":3},"045","检查作业- 安全带　　　　                                    \n- 检查驾驶员座椅安全带的拉伸和卷收情况及安全带有无撕裂或磨损"]
[{"$nulls":3},"046","检查作业- 安全带　　　　                                     \n- 检查驾驶员座椅安全带惯性开关和安全带扣锁止开关的工作情况"]
[{"$nulls":3},"047","拆装作业- 发动机                                                    \n- 拆下机油加注口盖"]
[{"$nulls":3},"048","检查作业- 发动机舱盖                                                       \n- 检查发动机舱盖锁和微开开关的工作情况"]
[{"$nulls":3},"049","检查作业- 车门      \n- 检查左后车门门锁（含儿童锁）和微开开关的工作情况"]
[{"$nulls":3},"050","检查作业- 车内灯                                                      \n- 检查行李箱照明灯是否点亮"]
[{"$nulls":3},"051","检查作业- 行李箱盖                               \n- 检查行李箱盖锁和微开开关的工作情况"]
[null,null,"填写附表","052","检查作业- 轮胎                                                   \n- 检测备用轮胎气压及轮胎是否漏气，必要时调整气压"]
[{"$nulls":3},"053","检查作业- 自动变速器\n- 检查换挡杆及挡位指示灯的工作情况，检查完毕后将换档杆置于N位置"]
[{"$nulls":3},"054","作业准备- 制动系统\n- 释放驻车制动杆"]
["以下是顶起位置2"]
[{"$nulls":3},"055","检查作业- 发动机 \n- 检查发动机各油封及结合面有无漏油 "]
[{"$nulls":3},"056","检查作业- 发动机\n- 检查机油滤清器及油底壳放油螺塞有无漏油"]
[{"$nulls":3},"057","拆装作业- 发动机润滑系统\n- 排放发动机机油"]
[{"$nulls":3},"058","检查作业- 发动机冷却系统                            \n- 检查散热器有无泄漏、脏污、变形或损坏"]
[{"$nulls":3},"059","检查作业- 传动系统\n- 检查左驱动轴护套有无泄漏、裂纹或损坏（外侧）"]
[{"$nulls":3},"060","检查作业- 传动系统\n- 检查右驱动轴护套有无泄漏、裂纹或损坏（外侧）"]
[{"$nulls":3},"061","检查作业- 转向系统\n- 检查左转向横拉杆防尘罩有无漏油、裂纹或损坏"]
[{"$nulls":3},"062","检查作业- 转向系统\n- 检查右转向横拉杆防尘罩有无漏油、裂纹或损坏"]
[{"$nulls":3},"063","检查作业- 燃油供给系统\n- 检查燃油管及接头有无泄漏"]
[{"$nulls":3},"064","检查作业- 燃油供给系统\n- 检查燃油管的安装情况及有无扭结、磨损、腐蚀或其他损坏"]
[{"$nulls":3},"065","检查作业- 制动系统\n- 检查制动管及接头有无泄漏"]
[{"$nulls":3},"066","检查作业- 制动系统\n- 检查制动管的安装情况及有无扭结、磨损、腐蚀或其他损坏"]
[{"$nulls":3},"067","检查作业- 排气系统\n- 检查三元催化器、排气管、消声器有无凹陷、刮伤、腐蚀或其他损坏"]
[{"$nulls":3},"068","检查作业- 排气系统\n- 检查排气系统各密封垫片有无泄漏"]
[{"$nulls":3},"069","检查作业- 排气系统\n- 检查排气管、消声器的吊挂有无裂纹、损坏、脱落或缺失"]
[{"$nulls":3},"070","紧固作业- 前副车架\n- 紧固前副车架与车身连接螺栓（后部）"]
[{"$nulls":3},"071","紧固作业- 后桥托架\n- 紧固后桥托架与车身连接螺栓（内侧）"]
[{"$nulls":3},"072","固作业- 后悬架\n- 紧固左后减振器下螺栓"]
[{"$nulls":3},"073","紧固作业- 后悬架\n- 紧固右后减振器下螺栓"]
[{"$nulls":3},"074","拆装作业- 发动机\n- 更换新的放油螺塞密封件并安装放油螺塞"]
["以下是顶起位置3"]
[{"$nulls":3},"075","检查作业- 前悬架                                                  \n- 检查左前减振器有无漏油、变形或其他损坏"]
[{"$nulls":3},"076","检查作业- 车轮\n- 检查左前车轮轴承有无松旷和异响"]
[{"$nulls":3},"077","拆装作业- 车轮\n- 拆卸左前车轮"]
[{"$nulls":3},"078","拆装作业- 制动系统 \n- 拆卸左前轮制动钳下部固定螺栓"]
[{"$nulls":3},"079","检查作业- 制动系统 \n- 检查左前轮制动钳导销是否松旷、导销护套有无裂纹或损坏"]
[{"$nulls":3},"080","检查作业- 制动系统\n- 检查左前轮制动钳活塞有无泄漏"]
[{"$nulls":3},"081","拆装作业- 制动系统\n- 用专用工具压回左前轮制动钳活塞"]
[{"$nulls":3},"082","拆装作业- 制动系统 \n- 拆卸并检查左前轮制动片固定弹簧有无变形、裂纹或损坏"]
[{"$nulls":3},"083","检查作业- 制动系统\n- 检查左前轮制动盘有无裂纹、沟槽或损坏"]
[null,null,"填写附表","084","检测作业- 制动系统 \n- 测量并记录左前轮制动盘横向跳动量"]
[{"$nulls":3},"085","拆装作业- 制动系统\n- 安装左前轮制动片固定弹簧"]
[{"$nulls":3},"086","拆装作业- 制动系统\n- 更换左前轮制动片"]
[{"$nulls":3},"087","拆装作业- 制动系统\n- 安装左前轮制动钳"]
[null,null,"填写附表","088","检测作业- 轮胎                                                    \n-检测并记录左后轮胎胎面沟槽深度"]
[{"$nulls":3},"089","拆装作业- 车轮\n- 拆下左后车轮总成"]
[{"$nulls":3},"090","拆装作业- 制动系统\n- 拆下左后轮制动鼓螺钉并取下制动鼓"]
[{"$nulls":3},"091","检查作业- 制动系统\n- 检查左后轮制动鼓表面状况"]
[null,null,"填写附表","092","检测作业- 制动系统\n- 测量并记录左后轮制动鼓直径"]
[{"$nulls":3},"093","检查作业- 制动系统 \n- 检查左后轮制动分泵有无漏油、护套有无裂纹和损坏"]
[{"$nulls":3},"094","检查作业- 制动系统 \n- 检查左后轮制动分泵活塞有无卡滞"]
[{"$nulls":3},"095","检查作业- 制动系统\n- 检查左后轮制动蹄摩擦衬片有无裂纹、缺损和油污"]
[null,null,"填写附表","096","检测作业- 制动系统\n- 测量并记录左后轮制动蹄直径，并计算其与制动鼓的间隙"]
[{"$nulls":3},"097","检查作业- 制动系统\n- 检查左后轮制动器调节弹簧有无缺失、弯曲、裂纹或严重锈蚀"]
[{"$nulls":3},"098","检查作业- 制动系统 \n- 检查左后轮制动器调节器总成有无弯曲、裂纹、过度磨损、损坏或缺齿"]
[{"$nulls":3},"099","拆装作业- 制动系统 \n- 安装左后轮制动鼓并紧固制动鼓螺钉"]
[{"$nulls":3},"100","调整作业- 制动系统\n- 恢复制动器盘片和蹄鼓的间隙"]
[{"$nulls":3},"101","检查作业- 制动系统                                                              \n- 检查左前制动盘转动是否灵活"]
[{"$nulls":3},"102","拆装作业- 制动系统                                                    \n- 进行左侧车轮前后换位，安装并预紧固左前车轮"]
[{"$nulls":3},"103","检查作业- 制动系统                                                              \n- 检查左后制动鼓转动是否灵活"]
[{"$nulls":3},"104","拆装作业- 制动系统                                                    \n- 进行左侧车轮前后换位，安装并预紧固左后车轮"]
[null,null,"填写附表","105","检查作业- 制动系统                                              \n- 检查并记录制动踏板的自由行程"]
[null,null,"填写附表","106","检查作业- 制动系统                                            \n- 检查并记录制动踏板的行程"]
[null,null,"填写附表","107","检查作业- 制动系统\n- 检查并记录驻车制动器拉杆的行程"]
[{"$nulls":3},"108","作业准备- 工量具和设备\n- 启动尾气分析仪                 "]
["以下是顶起位置4"]
[{"$nulls":3},"109","作业准备- 安全防护                                            \n- 拉紧驻车制动杆，并将换挡杆置于P位置"]
[{"$nulls":3},"110","作业准备- 安全防护\n- 安装车轮挡块"]
[{"$nulls":3},"111","紧固作业- 车轮             \n- 紧固左前车轮螺母","扭矩为80NM"]
[{"$nulls":3},"112","紧固作业- 车轮             \n- 紧固左后车轮螺母","扭矩为80NM"]
[{"$nulls":3},"113","拆装作业- 发动机润滑系统\n- 拆卸机油滤清器盖及其密封件"]
[{"$nulls":3},"114","拆装作业- 发动机润滑系统\n- 更换新的机油滤清器芯"]
[{"$nulls":3},"115","拆装作业- 发动机润滑系统 \n- 更换新的机油滤清器盖密封件并安装机油滤清器盖"]
[null,null,"填写附表","116","拆装作业- 发动机润滑系统\n- 加注新的发动机油并填写发动机机油更换记录表"]
[{"$nulls":3},"117","检查作业- 进气系统\n- 检查并清洁空气滤清器外壳"]
[{"$nulls":3},"118","拆装作业- 进气系统\n- 更换新的空气滤清器芯"]
[{"$nulls":3},"119","作业准备- 发动机\n- 起动发动机并暖机(及时观察发动机机油有无泄漏)"]
[{"$nulls":3},"120","检查作业- 制动系统                                          \n- 检查制动助力器的助力能力"]
[{"$nulls":3},"121","检查作业- 玻璃升降器                        \n- 检查主控制开关的玻璃升降控制功能","起动发动机"]
[{"$nulls":3},"122","检查作业- 车外后视镜                         \n- 检查右后视镜的调整功能"]
[{"$nulls":3},"123","检查作业- 空调\n- 检查风速调节和风向切换功能以及制冷系统能否工作","起动发动机"]
[null,null,"填写附表","124","检查作业- 电源系统\n- 进行充电系统测试，并记录蓄电池充电电压"]
[null,null,"填写附表","125","检测作业- 发动机排气系统 \n- 检测并记录发动机怠速时的尾气排放值"]
["以下是顶起位置5"]
[{"$nulls":3},"126","检查作业- 发动机                                                              \n- 检查发动机机油有无泄漏"]
[{"$nulls":3},"127","检查作业- 发动机                                                              \n- 检查冷却液有无泄漏"]
[{"$nulls":3},"128","检查作业- 制动系统                                                               \n- 检查左前和左后部有无制动液泄漏"]
["以下是顶起位置6"]
[{"$nulls":3},"129","整理作业- 工量具和设备\n- 关闭尾气分析仪并清洁归位"]
[{"$nulls":3},"130","检查作业- 发动机润滑系统\n- 检查发动机机油液位，必要时调整"]
[{"$nulls":3},"131","整理作业- 工量具和设备\n- 清洁工量具和设备并归位"]
[{"$nulls":3},"132","整理作业- 安全防护                                                               \n- 拆卸翼子板布和前格栅布"]
[{"$nulls":3},"133","整理作业- 安全防护                                                               \n- 拆卸座椅套、地板垫、方向盘套"]
[{"$nulls":3},"134","清洁作业- 车身                                                              \n- 清洁车辆内部、烟灰缸等"]
[{"$nulls":3},"135","清洁作业- 车身                                                              \n- 清洁车辆外表"]
[]
["说明：",null,"对于不合格的作业项目，要在维修工单内写明故障点，并勾选相应的维修措施；记录项划斜杠的，无需记录；记录项中标明填写附表的，按附表的要求填写。"]